{"text_format":"3","workbook":"xls","n_sheets":5,"sheets":["Power and Cooling","Rotor HP","Cooling Calculations","Manifold Pressure","Performance"],"not_rendered":{"macros":1,"external_links":2,"defined_names":30,"comments":8},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Power and Cooling","index":0,"n_rows":56,"n_cols":23,"rows_kept":56,"merged":[[5,2,5,7],[6,2,6,7],[6,11,7,11],[7,2,7,7],[7,17,10,17],[7,18,10,18],[8,2,8,7],[9,2,9,7],[9,10,10,10],[9,11,10,11],[9,12,10,12],[9,13,10,13],[9,14,10,14],[9,15,10,15],[9,16,10,16],[10,2,10,7],[16,2,21,8],[36,2,37,3]],"flags":["formulas_cached_only"]}
[]
[null,null,"Power and Heat Rejection Requirements Calculator",{"$nulls":14},"Results"]
[null,null," ",null,"Rotary Engine",{"$nulls":5},"AF =",12.65,"Temp F =",59,null," "]
[{"$nulls":10},"Gear Ratio =",2.17,"Manifold",{"v":29,"d":"29.00"},"\"Hg"," "]
[{"$nulls":10},"Number Rotors =",2]
[null,null,"Air Fuel Mixture Ratio(Air Part)",{"$nulls":5},12.65,12.65]
[null,null,"Initial Engine RPM",{"$nulls":5},5500,5000,null,"Prop Torque",{"$nulls":3}," Engine Torque ",null," "," "]
[null,null,"RPM Step",{"$nulls":5},100,100,{"$nulls":5},"(max rpm)",null,"Radiator  Heat Rejection Requirement BTU/Minute","Oil Cooler Heat Rejection Requirements BTU/Minute"]
[null,null,"Manifold Pressure Inches Mercury \" Hg",{"$nulls":5},{"v":29,"d":"29.00"},29.92,null,{"v":316.2611155271788,"d":"316"},{"$nulls":3},{"v":145.7424495516953,"d":"146"}]
[null,null,"Enter Air Temperature(Select -15F->100F)",{"$nulls":5},59,59,"Engine RPM","Prop RPM","Air Flow CFM","Air Mass lbm/Min","Fuel Flow Lbm/min","Horse Power ","Gallon/Hour"]
[null,null,"Turbo",{"$nulls":5},"No","NO"]
[null,null,"Message:  ","",{"$nulls":4}," ",null,5500,{"v":2534.562211981567,"d":"2535"},{"v":241.89814814814815,"d":"241.9"},{"v":17.95907906431803,"d":"17.96"},{"v":1.4196900446101208,"d":"1.42"},{"v":152.6244235594677,"d":"153"},{"v":14.196900446101209,"d":"14.2"},{"v":4675.512546915998,"d":"4676"},{"v":2337.756273457999,"d":"2338"}]
[null,null,"Number Rotors",{"$nulls":5},2,2,5600,{"v":2580.6451612903224,"d":"2581"},{"v":246.2962962962963,"d":"246.3"},{"v":18.28560777457836,"d":"18.29"},{"v":1.4455025908757597,"d":"1.45"},{"v":155.39941307873076,"d":"155"},{"v":14.455025908757598,"d":"14.5"},{"v":4760.5218659508355,"d":"4761"},{"v":2380.2609329754177,"d":"2380"}]
[null,null,"Gear Ratio ",{"$nulls":5},2.17,2.17,5700,{"v":2626.7281105990783,"d":"2627"},{"v":250.69444444444446,"d":"250.7"},{"v":18.612136484838686,"d":"18.61"},{"v":1.4713151371413982,"d":"1.47"},{"v":158.17440259799378,"d":"158"},{"v":14.713151371413982,"d":"14.7"},{"v":4845.531184985671,"d":"4846"},{"v":2422.7655924928354,"d":"2423"}]
[{"$nulls":10},5800,{"v":2672.811059907834,"d":"2673"},{"v":255.0925925925926,"d":"255.1"},{"v":18.938665195099013,"d":"18.94"},{"v":1.4971276834070366,"d":"1.50"},{"v":160.94939211725682,"d":"161"},{"v":14.971276834070366,"d":"15.0"},{"v":4930.540504020507,"d":"4931"},{"v":2465.2702520102534,"d":"2465"}]
[null,null,"Version 3.0  Copyright Oct 2007 by Edward L. Anderson",{"$nulls":7},5900,{"v":2718.89400921659,"d":"2719"},{"v":259.49074074074076,"d":"259.5"},{"v":19.265193905359343,"d":"19.27"},{"v":1.5229402296726753,"d":"1.52"},{"v":163.72438163651992,"d":"164"},{"v":15.229402296726754,"d":"15.2"},{"v":5015.549823055345,"d":"5016"},{"v":2507.7749115276724,"d":"2508"}]
[null,null,"FOR EDUCATIONAL AND ENTERTAINMENT PURPOSES ONLY                                                                      This spreadsheet is designed to provide first order estimates of engine power and BTU Heat rejection requirements for a Mazda Wankel 13B Normally aspired engine. It will provide an estimate for Sea Level Power and Power at Altitude MSL. Note: Engine load is not a computational factor, but can be approximated to some degree by manifold pressure.  Enter your desired parameters in the blue Data Input Box.  Copywrite @ January, 19, 1994",{"$nulls":7},6000,{"v":2764.9769585253457,"d":"2765"},{"v":263.88888888888886,"d":"263.9"},{"v":19.591722615619666,"d":"19.59"},{"v":1.5487527759383135,"d":"1.55"},{"v":166.4993711557829,"d":"166"},{"v":15.487527759383134,"d":"15.5"},{"v":5100.55914209018,"d":"5101"},{"v":2550.27957104509,"d":"2550"}]
[{"$nulls":10},6100,{"v":2811.0599078341015,"d":"2811"},{"v":268.287037037037,"d":"268.3"},{"v":19.918251325879993,"d":"19.92"},{"v":1.574565322203952,"d":"1.57"},{"v":169.27436067504593,"d":"169"},{"v":15.74565322203952,"d":"15.7"},{"v":5185.568461125015,"d":"5186"},{"v":2592.7842305625077,"d":"2593"}]
[{"$nulls":10},6200,{"v":2857.1428571428573,"d":"2857"},{"v":272.68518518518516,"d":"272.7"},{"v":20.244780036140323,"d":"20.24"},{"v":1.6003778684695908,"d":"1.60"},{"v":172.04935019430903,"d":"172"},{"v":16.00377868469591,"d":"16.0"},{"v":5270.577780159852,"d":"5271"},{"v":2635.288890079926,"d":"2635"}]
[{"$nulls":10},6300,{"v":2903.225806451613,"d":"2903"},{"v":277.0833333333333,"d":"277.1"},{"v":20.57130874640065,"d":"20.57"},{"v":1.6261904147352293,"d":"1.63"},{"v":174.82433971357204,"d":"175"},{"v":16.261904147352293,"d":"16.3"},{"v":5355.5870991946895,"d":"5356"},{"v":2677.7935495973447,"d":"2678"}]
[{"$nulls":10},6400,{"v":2949.308755760369,"d":"2949"},{"v":281.48148148148147,"d":"281.5"},{"v":20.897837456660977,"d":"20.90"},{"v":1.6520029610008677,"d":"1.65"},{"v":177.59932923283512,"d":"178"},{"v":16.520029610008677,"d":"16.5"},{"v":5440.596418229526,"d":"5441"},{"v":2720.298209114763,"d":"2720"},null,null," "," "]
[{"$nulls":10},6500,{"v":2995.3917050691243,"d":"2995"},{"v":285.8796296296296,"d":"285.9"},{"v":21.224366166921307,"d":"21.22"},{"v":1.6778155072665064,"d":"1.68"},{"v":180.37431875209816,"d":"180"},{"v":16.77815507266506,"d":"16.8"},{"v":5525.605737264362,"d":"5526"},{"v":2762.802868632181,"d":"2763"}]
[]
[{"$nulls":4}," ",{"$nulls":7}," ",null," ",{"$nulls":6},"  "]
[{"$nulls":3},"  ",{"$nulls":5}," "," "]
[{"$nulls":4},"Cooling Capacity Calculator",{"$nulls":13},"Radiator/Cooler Data"]
[{"$nulls":22},"GM evaporator core - Width = 10.5, Height = 9.0 inches"]
[{"$nulls":3},"Note Cooling Capacity is based on two GM evaporator cores and one stock RX-7 Oil cooler",{"$nulls":15},"Enter Surface Area Data",null,null,"two normally used."]
[{"$nulls":3},"(Note: RPM Entered must appear in RESULTS Table - change RPM starting point or step increment to ensure this- if required)",{"$nulls":15},"Fin Area Only",null,null,"Note:  Cooling capacity based soley on Mass flow"]
[{"$nulls":3},"(This rpm should represent the RPM you encounter or expect for the Regime of flight you are in such as Take-0ff, Climb, Cruise, etc)",{"$nulls":15},"Width (nches)",11,null,"through radiator surface area which can be affected by"]
[{"$nulls":3},"(For example your RPM on climbout may be 5600 rpm but your airspeed may only be 120 MPH indicated, where as you may still)",{"$nulls":15},"Height(Inches)",9,null,"a number of factors not taken into consideration in"]
[{"$nulls":3},"(Have an engine rpm of 5600 at cruise, but your airspeed would be more like 170 MPH Indicated.)",{"$nulls":15}," ",null,null,"this simple cooling capacity calculator"]
[{"$nulls":3},"(The selection of this rpm is important for the cooling calculation as it determines the BTU of waste heat rejection required)",{"$nulls":15},"Number of Rads",2,null,"Number of radiators of size entered"]
[{"$nulls":19},"Number of Oil Coolers     ",1,null,"Note: Oil coolers are assumed to be stock RX-7"]
[null,null,"Indicated Air Speed ",null,120,"MPH","",null,null,"Total Cooling Capacity (Radiators and oil Cooler)"]
[null,null,"Altitude MSL",null,100,"Feet"]
[null,null,"Engine RPM of Operating Regime",null,6000,"RPM","HP","Fuel GPH",null,null,"Total Heat Rejection Capacity",null,null,{"v":7810.039709009999,"d":"7810"},"BTU/Minute",{"$nulls":4}," "]
[{"$nulls":6},{"v":166.4993711557829,"d":"166"},{"v":15.487527759383134,"d":"15.49"},{"$nulls":10}," "," "]
[{"$nulls":10},"Total Heat Rejection Requried",null,null,{"v":7650.83871313527,"d":"7651"},"BTU/Minute"]
[]
[{"$nulls":10},"Overall System Cooling Status",null,null,"Cooling",""]
[]
[{"$nulls":10},"Delta Capacity",null,null,{"v":0.020808306362726715,"d":"2.08%"},{"$nulls":5}," "]
[]
[{"$nulls":19}," "]
[null,null,"Radiator Data",{"$nulls":6},"Oil Cooler Data",{"$nulls":9}," "]
[]
[null,null,"Heat Rejection Data",{"$nulls":6},"Heat Rejection Data"]
[]
[{"$nulls":3},"Heat Rejection Capability ",null,null,{"v":5294.942175599999,"d":"5295"},"BTU/Minute "," ",null,"Heat Rejection Capability ",null,null,{"v":2515.0975334099994,"d":"2515"},"BTU/Minute ",null," ",null,null," "]
[{"$nulls":6}," "," ",{"$nulls":5}," "," ",{"$nulls":5}," "," "]
[{"$nulls":3},"Heat Rejection Required ",null,null,{"v":5100.55914209018,"d":"5101"},"BTU/Minute "," ",null,"Heat Rejection Required ",null,null,{"v":2550.27957104509,"d":"2550"},"BTU/Minute",null," ",null,null," "," "," "]
[]
[{"$nulls":3},"Cooling Status",null,null,"Cooling","",null,null,"Cooling Status",null,null,"","Overheating"]
[]
[{"$nulls":3},"Delta Capacity",null,null,{"v":0.03811014206378991,"d":"3.81%"},{"$nulls":3},"Delta Capacity",null,null,{"v":-0.013795365039399677,"d":"-1.38%"}]

{"sheet":"Rotor HP","index":1,"n_rows":153,"n_cols":46,"rows_kept":153,"hidden":true,"merged":[[0,2,0,10],[1,2,1,10],[1,15,1,17],[2,3,2,9],[3,2,3,9],[5,3,5,8],[5,13,6,13],[5,17,6,17],[5,18,6,18],[6,3,6,8],[7,3,7,8],[8,3,8,8],[9,3,9,8],[10,3,10,8],[11,3,11,8],[23,3,23,4],[24,3,24,4],[25,3,25,4],[26,3,26,4],[74,17,74,18],[77,0,78,0],[89,6,89,8],[89,13,89,15],[90,6,90,8],[90,13,90,15],[91,6,91,8],[91,13,91,15],[92,6,92,8],[92,13,92,15],[93,6,93,8],[93,13,93,15],[94,6,94,8],[94,13,94,15],[95,13,95,15],[96,13,96,15],[97,13,97,15],[98,13,98,15],[99,13,99,15],[100,13,100,15],[101,13,101,15],[102,13,102,15],[103,13,103,15],[104,13,104,15],[105,13,105,15],[106,13,106,15],[107,13,107,15],[108,13,108,15],[109,13,109,15],[110,13,110,15],[111,13,111,15],[112,13,112,15],[113,13,113,15],[115,17,118,18],[127,8,127,9],[128,8,128,9]],"flags":["formulas_cached_only"]}
[null,null,"Mazda Wankel Rotary Engine Performance Spreadsheet Version 1.5 Mar 2001"]
[null,null,"  FOR EDUCATIONAL AND ENTERTAINMENT PURPOSES ONLY                                                                      This spreadsheet is designed to provide first order estimates of engine power and BTU Heat rejection requirements for a Mazda Wankel 13B Normally aspired engine. It will provide an estimate for Sea Level Power and Power at Altitude MSL. Note: Engine load is not a computational factor, but can be approximated to some degree by varying the throttle setting.  Enter your desired parameters in the blue Data Input Box.  Copywrite @ January, 19, 1994",{"$nulls":12},"Calculation Results"]
[null," ",{"$nulls":11},"AF =",12.65," ","Temp F =",59]
[null,null,"Developed by: Ed Anderson, eanderson@carolina.rr.com, Matthews NC",{"$nulls":10},"Altitude =",100," ","Manifold",{"v":29,"d":"29.00"}]
[{"$nulls":3},"This Spreadsheet is Protected to Preclude Inadvertent erasing of Formulas",{"$nulls":9},"Gear Ratio =",2.17,null,"RESULTS"]
[null,"Default Values",null,"DATA ENTRY BOX",{"$nulls":5}," Enter Data",{"$nulls":3},"Engine RPM",{"$nulls":3},"Radiator Cooler Heat Rejection Requirement BTU/Minute","Oil Cooler Heat Rejection Requirements BTU/Minute"]
[null,13.5,null,"Air Fuel Mixture Ratio(Air Part)",{"$nulls":5},12.65,{"$nulls":4},"Prop RPM","Horse Power/Sec","Gallon/Hour"]
[null,4000,null,"Initial Engine RPM",{"$nulls":5},5500]
[null,250,null,"RPM Step",{"$nulls":5},100,{"$nulls":3},5500,{"v":2534.562211981567,"d":"2535"},{"v":152.6244235594677,"d":"153"},{"v":14.196900446101209,"d":"14.20"},{"v":4675.512546915998,"d":"4676"},{"v":2337.756273457999,"d":"2338"}," "]
[null,100,null,"% Throttle Opening (Enter Percentage)",{"$nulls":5},{"v":29,"d":"2900%"},{"$nulls":3},5600,{"v":2580.6451612903224,"d":"2581"},{"v":155.39941307873076,"d":"155"},{"v":14.455025908757598,"d":"14.46"},{"v":4760.5218659508355,"d":"4761"},{"v":2380.2609329754177,"d":"2380"}]
[null,0,null,"MSL Altitude in feet",{"$nulls":5},100,{"$nulls":3},5700,{"v":2626.7281105990783,"d":"2627"},{"v":158.17440259799378,"d":"158"},{"v":14.713151371413982,"d":"14.71"},{"v":4845.531184985671,"d":"4846"},{"v":2422.7655924928354,"d":"2423"}]
[null,60,null,"Enter Air Temperature (Select 15F - 100F, in 5 Degree  Increments)",{"$nulls":5},59,{"$nulls":3},5800,{"v":2672.811059907834,"d":"2673"},{"v":160.94939211725682,"d":"161"},{"v":14.971276834070366,"d":"14.97"},{"v":4930.540504020507,"d":"4931"},{"v":2465.2702520102534,"d":"2465"}]
[null,{"v":0,"d":"0.000"},null,"Enter Boost (psi Gauge)  Calculations Compensate for Altitude",{"$nulls":5},0,0.9991596638655463,null,null,5900,{"v":2718.89400921659,"d":"2719"},{"v":163.72438163651992,"d":"164"},{"v":15.229402296726754,"d":"15.23"},{"v":5015.549823055345,"d":"5016"},{"v":2507.7749115276724,"d":"2508"}]
[{"$nulls":13},6000,{"v":2764.9769585253457,"d":"2765"},{"v":166.4993711557829,"d":"166"},{"v":15.487527759383134,"d":"15.49"},{"v":5100.55914209018,"d":"5101"},{"v":2550.27957104509,"d":"2550"}]
[{"$nulls":3},"Step 1 Enter Air/Fuel Ratio (Air Value)",{"$nulls":9},6100,{"v":2811.0599078341015,"d":"2811"},{"v":169.27436067504593,"d":"169"},{"v":15.74565322203952,"d":"15.75"},{"v":5185.568461125015,"d":"5186"},{"v":2592.7842305625077,"d":"2593"}]
[{"$nulls":3},"Step 2 Enter RPM Start Value",{"$nulls":9},6200,{"v":2857.1428571428573,"d":"2857"},{"v":172.04935019430903,"d":"172"},{"v":16.00377868469591,"d":"16.00"},{"v":5270.577780159852,"d":"5271"},{"v":2635.288890079926,"d":"2635"}]
[{"$nulls":3},"Step 3 Enter RPM Step Increment",{"$nulls":9},6300,{"v":2903.225806451613,"d":"2903"},{"v":174.82433971357204,"d":"175"},{"v":16.261904147352293,"d":"16.26"},{"v":5355.5870991946895,"d":"5356"},{"v":2677.7935495973447,"d":"2678"}," "]
[{"$nulls":3},"Step 4 Enter Throttle Opening %",{"$nulls":9},6400,{"v":2949.308755760369,"d":"2949"},{"v":177.59932923283512,"d":"178"},{"v":16.520029610008677,"d":"16.52"},{"v":5440.596418229526,"d":"5441"},{"v":2720.298209114763,"d":"2720"}]
[{"$nulls":3},"Step 5 Enter MSL Operating Altitude in thousand of feet",{"$nulls":9},6500,{"v":2995.3917050691243,"d":"2995"},{"v":180.37431875209816,"d":"180"},{"v":16.77815507266506,"d":"16.78"},{"v":5525.605737264362,"d":"5526"},{"v":2762.802868632181,"d":"2763"}]
[{"$nulls":3},"Step 6 Enter OAT F between 15 -100 in 5 degree increments",{"$nulls":9},6600,{"v":3041.47465437788,"d":"3041"},{"v":183.14930827136124,"d":"183"},{"v":17.036280535321453,"d":"17.04"},{"v":5610.6150562992,"d":"5611"},{"v":2805.3075281496,"d":"2805"}]
[{"$nulls":3},"Step 7 Enter Gauge Boost in PSI (Note: No intercooler in calculation)",{"$nulls":9},6700,{"v":3087.557603686636,"d":"3088"},{"v":185.92429779062425,"d":"186"},{"v":17.294405997977837,"d":"17.29"},{"v":5695.624375334035,"d":"5696"},{"v":2847.8121876670175,"d":"2848"}]
[{"$nulls":13},6800,{"v":3133.6405529953918,"d":"3134"},{"v":188.69928730988732,"d":"189"},{"v":17.552531460634224,"d":"17.55"},{"v":5780.63369436887,"d":"5781"},{"v":2890.316847184435,"d":"2890"}]
[{"$nulls":3},"NOTES  Below"]
[{"$nulls":3},"Number of Rotors",{"$nulls":4}," ",null," "]
[{"$nulls":3},"Fuel Injection Parameters Note"]
[{"$nulls":3},"Power Assumptions"]
[{"$nulls":3},"Assumed Max Power",{"$nulls":12},"Manifold Pressure/Power Estimates"]
[{"$nulls":15}," ",null,100]
[{"$nulls":13}," Assumed Max Engine Power",null,180,"Temp F",59,"Specified Max RPM for Look Up Table",6400]
[{"$nulls":13},"A/F Ratio",null,12.65,"Altitude","8000 Ft","Throttle",{"v":29,"d":"2900%"}]
[{"$nulls":15},"% Engine Power","HP","Inches HG","RPM"]
[{"$nulls":15},{"v":0.9866629401824173,"d":"99%"},{"v":177.59932923283512,"d":"178"},22,6400," "]
[{"$nulls":15},{"v":0.9418146247195802,"d":"94%"},{"v":169.52663244952444,"d":"170"},21,{"v":6109.090909090909,"d":"6109"}]
[{"$nulls":15},{"v":0.896966309256743,"d":"90%"},{"v":161.45393566621374,"d":"161"},20,{"v":5818.181818181819,"d":"5818"}]
[{"$nulls":15},{"v":0.8521179937939058,"d":"85%"},{"v":153.38123888290306,"d":"153"},19,{"v":5527.272727272727,"d":"5527"}]
[{"$nulls":15},{"v":0.8072696783310688,"d":"81%"},{"v":145.3085420995924,"d":"145"},18,{"v":5236.363636363637,"d":"5236"}]
[{"$nulls":15},{"v":0.7624213628682316,"d":"76%"},{"v":137.23584531628168,"d":"137"},17,{"v":4945.454545454546,"d":"4945"}]
[{"$nulls":15},{"v":0.7175730474053945,"d":"72%"},{"v":129.163148532971,"d":"129"},16,{"v":4654.545454545455,"d":"4655"}]
[{"$nulls":15},{"v":0.6727247319425572,"d":"67%"},{"v":121.0904517496603,"d":"121"},15,{"v":4363.636363636363,"d":"4364"}]
[{"$nulls":15},{"v":0.62787641647972,"d":"63%"},{"v":113.01775496634961,"d":"113"},14,{"v":4072.7272727272725,"d":"4073"}]
[{"$nulls":15},{"v":0.583028101016883,"d":"58%"},{"v":104.94505818303894,"d":"105"},13,{"v":3781.818181818182,"d":"3782"}]
[{"$nulls":15},{"v":0.5381797855540458,"d":"54%"},{"v":96.87236139972823,"d":"97"},12,{"v":3490.9090909090905,"d":"3491"}]
[{"$nulls":15},{"v":0.49333147009120865,"d":"49%"},{"v":88.79966461641756,"d":"89"},11,3200]
[{"$nulls":15},{"v":0.4484831546283715,"d":"45%"},{"v":80.72696783310687,"d":"81"},10,{"v":2909.0909090909095,"d":"2909"}]
[{"$nulls":15},{"v":0.4036348391655344,"d":"40%"},{"v":72.6542710497962,"d":"73"},9,{"v":2618.1818181818185,"d":"2618"}]
[{"$nulls":15},{"v":0.35878652370269726,"d":"36%"},{"v":64.5815742664855,"d":"65"},8,{"v":2327.2727272727275,"d":"2327"}]
[{"$nulls":15},{"v":0.31393820823986,"d":"31%"},{"v":56.50887748317481,"d":"57"},7,{"v":2036.3636363636363,"d":"2036"}]
[{"$nulls":15},{"v":0.2690898927770229,"d":"27%"},{"v":48.43618069986412,"d":"48"},6,{"v":1745.4545454545453,"d":"1745"}]
[{"$nulls":15},{"v":0.22424157731418576,"d":"22%"},{"v":40.363483916553434,"d":"40"},5,{"v":1454.5454545454547,"d":"1455"}]
[{"$nulls":15},{"v":0.17939326185134863,"d":"18%"},{"v":32.29078713324275,"d":"32"},4,{"v":1163.6363636363637,"d":"1164"}]
[{"$nulls":15},{"v":0.13454494638851144,"d":"13%"},{"v":24.21809034993206,"d":"24"},3,{"v":872.7272727272726,"d":"873"}]
[{"$nulls":15},{"v":0.08969663092567431,"d":"9%"},{"v":16.145393566621376,"d":"16"},2,{"v":581.8181818181819,"d":"582"}]
[{"$nulls":15},{"v":0.04484831546283716,"d":"4%"},{"v":8.072696783310688,"d":"8"},1,{"v":290.90909090909093,"d":"291"}]
[{"$nulls":15},{"v":0,"d":"0%"},0,0,0]
[{"$nulls":15},{"v":-0.04484831546283716,"d":"-4%"},{"v":-8.072696783310688,"d":"-8"},-1,{"v":-290.90909090909093,"d":"-291"}]
[{"$nulls":15},{"v":-0.08969663092567431,"d":"-9%"},{"v":-16.145393566621376,"d":"-16"},-2,{"v":-581.8181818181819,"d":"-582"}]
[{"$nulls":15},{"v":-0.13454494638851144,"d":"-13%"},{"v":-24.21809034993206,"d":"-24"},-3,{"v":-872.7272727272726,"d":"-873"}]
[{"$nulls":15},{"v":-0.17939326185134863,"d":"-18%"},{"v":-32.29078713324275,"d":"-32"},-4,{"v":-1163.6363636363637,"d":"-1164"}]
[{"$nulls":15},{"v":-0.22424157731418576,"d":"-22%"},{"v":-40.363483916553434,"d":"-40"},-5,{"v":-1454.5454545454547,"d":"-1455"}]
[{"$nulls":15},{"v":-0.2690898927770229,"d":"-27%"},{"v":-48.43618069986412,"d":"-48"},-6,{"v":-1745.4545454545453,"d":"-1745"}]
[]
[]
[]
[]
[]
[]
[{"$nulls":13},"Calculation Parameters and Equations"]
[]
[]
[{"$nulls":22}," "," "]
[null,"Turbo Charger Density Compensation",{"$nulls":16}," ",{"$nulls":3}," "]
["P1 At Altitude",{"v":14.689655172413795,"d":"14.69"},29.898944405348352,29.82," "," ",{"$nulls":3},"Spreadsheet for calculating Engine Power, BTU cooling, and injector Timing",{"$nulls":12}," "]
["P2 psi Gauge",0,0,1,0,{"$nulls":4},"Parameter","Units","Value","Air Density                                                    Factor","Conversion Values",{"$nulls":3},"Engines 13B (2 Rotors) , 20G (3 Rotors)",{"$nulls":4}," "]
[2.035374149659864,{"$nulls":6},"=L74*(-3*10^(-5)*$J$11+1)",null,"Air Mass Pa (Sea Level)","Lbm/Ft^3",0.076636,0.0023799999999999997,"Gasoline Energy",null,null,"19000 Btu/lbm-sec","VC=Rotor Chamber volume CID",null,{"v":40,"d":"40.000"}," "]
[null,null,"Delta T Ideal",null,"Delta T Real",{"$nulls":3},"Compensate for altitude ","Air Mass Pa  (Altitude MSL) ","Lbm/Ft^3",{"v":0.076406092,"d":"0.076406"},1.0008410428931875,"1 Btu =",null,null,"778 ft-lb","R = Number of Rotors",null,{"v":2,"d":"2.000"}," ",{"$nulls":3}," "]
["T1 Inlet Temp F",59,0,null,0,null,null,{"v":0.076406092,"d":"0.076406"},null,"Fuel Mass Pf","Lbm/Ft^3",44.883,null,"1 Horse Power =",null,null,"550 ft-lb ","F = Faces Per Rotor",null,{"v":3,"d":"3.000"}]
[{"$nulls":9},"Temperature","Degrees F",null,{"v":59,"d":"59.000"},{"$nulls":4},"Total Swept Chamber Volume per Rotor Rev - Single Rotor",null,{"v":120,"d":"120.000"},"Read Note -->"]
["Compressor Efficiency",65,{"$nulls":7},"Fuel/Air Ratio",null,{"v":0.07905138339920949,"d":"0.079"},{"$nulls":5},"VCID=Total Displacement for N rotors per Rotor rev",null,{"v":240,"d":"240.000"},{"$nulls":4}," "]
[{"$nulls":8}," ","  Fuel",null,{"v":1,"d":"1.000"},{"$nulls":5},"AirDisplacement per Rotor Revolution (Cubic Feet)",null,{"v":0.1388888888888889,"d":"0.139"},{"$nulls":3}," "]
[{"$nulls":9},"  Air",null,null,{"v":12.65,"d":"12.650"}]
["T2 Oulet Temp F",59,{"$nulls":6}," "]
[{"$nulls":9},"Engine RPM/Airflow Calculations",{"$nulls":9}," "]
[{"$nulls":21}," "]
[null,null,"Temp Ratio","Pressure Ratio",{"$nulls":5},"Operating parameters",null," ",{"$nulls":7}," "]
["Density Ratio",1,1,1,{"$nulls":5},"Intake 'Efficiency Ve",null,null,{"v":0.95,"d":"95.00%"},"was 100%"]
[{"$nulls":9},"Vt Throttle % Open",null,{"v":0.9687655577045117,"d":"0.969"},{"v":0.9687655577045117,"d":"96.88%"},"was Thottle % open"]
["Sea level air Density",0.076636,{"$nulls":7},"RPM Start Value",null,null,{"v":5500,"d":"5500.000"}]
[{"$nulls":9},"RPM Step Value",null,null,{"v":100,"d":"100.000"}," "]
["Altitude Density",{"v":0.076406092,"d":"0.076"}]
["Turbo Density",0.076406092,{"$nulls":4},"Once parameters are set for",null,null,"Engine RPM (Calculation",{"$nulls":3},"Eng RPM",null,null,5500,5600,5700,5800,5900,6000,6100,6200,6300,6400,6500,6600,6700,6800,null,"RPM",5500,5600,5700,5800,5900,6000,6100,6200,6300,6400,6500,6600,6700,6800]
[{"$nulls":6},"an engine configuration then",null,null,"Propeller RPM (PSRU Ratio = 2.17)",{"v":2.17,"d":"2.170"},null,null,"Prop RPM",null,null,{"v":2534.562211981567,"d":"2535"},{"v":2580.6451612903224,"d":"2581"},{"v":2626.7281105990783,"d":"2627"},{"v":2672.811059907834,"d":"2673"},{"v":2718.89400921659,"d":"2719"},{"v":2764.9769585253457,"d":"2765"},{"v":2811.0599078341015,"d":"2811"},{"v":2857.1428571428573,"d":"2857"},{"v":2903.225806451613,"d":"2903"},{"v":2949.308755760369,"d":"2949"},{"v":2995.3917050691243,"d":"2995"},{"v":3041.47465437788,"d":"3041"},{"v":3087.557603686636,"d":"3088"},{"v":3133.6405529953918,"d":"3134"},null,"AirFlow CFM",{"v":241.89814814814815,"d":"242"},{"v":246.2962962962963,"d":"246"},{"v":250.69444444444446,"d":"251"},{"v":255.0925925925926,"d":"255"},{"v":259.49074074074076,"d":"259"},{"v":263.88888888888886,"d":"264"},{"v":268.287037037037,"d":"268"},{"v":272.68518518518516,"d":"273"},{"v":277.0833333333333,"d":"277"},{"v":281.48148148148147,"d":"281"},{"v":285.8796296296296,"d":"286"},{"v":290.27777777777777,"d":"290"},{"v":294.6759259259259,"d":"295"},{"v":299.0740740740741,"d":"299"}]
[{"$nulls":6},"Normally only need to vary RPM",null,null,"Air Flow CFM",null,null," ","Air Flow CFM",null,null,{"v":241.89814814814815,"d":"242"},{"v":246.2962962962963,"d":"246"},{"v":250.69444444444446,"d":"251"},{"v":255.0925925925926,"d":"255"},{"v":259.49074074074076,"d":"259"},{"v":263.88888888888886,"d":"264"},{"v":268.287037037037,"d":"268"},{"v":272.68518518518516,"d":"273"},{"v":277.0833333333333,"d":"277"},{"v":281.48148148148147,"d":"281"},{"v":285.8796296296296,"d":"286"},{"v":290.27777777777777,"d":"290"},{"v":294.6759259259259,"d":"295"},{"v":299.0740740740741,"d":"299"},null,"Runner Dia (inches)",{"v":1.25,"d":"1.250"},{"v":1.25,"d":"1.250"},{"v":1.25,"d":"1.250"},{"v":1.25,"d":"1.250"},{"v":1.25,"d":"1.250"},{"v":1.25,"d":"1.250"},{"v":1.25,"d":"1.250"},{"v":1.25,"d":"1.250"},{"v":1.25,"d":"1.250"},{"v":1.25,"d":"1.250"},{"v":1.25,"d":"1.250"},{"v":1.25,"d":"1.250"},{"v":1.25,"d":"1.250"},{"v":1.25,"d":"1.250"}]
[{"$nulls":6},"Throttle Opening and  ",null,null,"Air Flow Lbm/min",null," "," ","Air Flow Mass",null,null,{"v":17.95907906431803,"d":"17.96"},{"v":18.28560777457836,"d":"18.29"},{"v":18.612136484838686,"d":"18.61"},{"v":18.938665195099013,"d":"18.94"},{"v":19.265193905359343,"d":"19.27"},{"v":19.591722615619666,"d":"19.59"},{"v":19.918251325879993,"d":"19.92"},{"v":20.244780036140323,"d":"20.24"},{"v":20.57130874640065,"d":"20.57"},{"v":20.897837456660977,"d":"20.90"},{"v":21.224366166921307,"d":"21.22"},{"v":21.550894877181634,"d":"21.55"},{"v":21.877423587441964,"d":"21.88"},{"v":22.20395229770229,"d":"22.20"},null,"Number Runners",{"v":2,"d":"2.00"},{"v":2,"d":"2.00"},{"v":2,"d":"2.00"},{"v":2,"d":"2.00"},{"v":2,"d":"2.00"},{"v":2,"d":"2.00"},{"v":2,"d":"2.00"},{"v":2,"d":"2.00"},{"v":2,"d":"2.00"},{"v":2,"d":"2.00"},{"v":2,"d":"2.00"},{"v":2,"d":"2.00"},{"v":2,"d":"2.00"},{"v":2,"d":"2.00"}]
[{"$nulls":6},"Perhaps fuel ratio",null,null,"Fuel Required LBM/Min",{"$nulls":3},"Fuel Flow Mass",null,null,{"v":1.4196900446101208,"d":"1.42"},{"v":1.4455025908757597,"d":"1.45"},{"v":1.4713151371413982,"d":"1.47"},{"v":1.4971276834070366,"d":"1.50"},{"v":1.5229402296726753,"d":"1.52"},{"v":1.5487527759383135,"d":"1.55"},{"v":1.574565322203952,"d":"1.57"},{"v":1.6003778684695908,"d":"1.60"},{"v":1.6261904147352293,"d":"1.63"},{"v":1.6520029610008677,"d":"1.65"},{"v":1.6778155072665064,"d":"1.68"},{"v":1.703628053532145,"d":"1.70"},{"v":1.7294405997977838,"d":"1.73"},{"v":1.7552531460634222,"d":"1.76"},null,"Runner Air Velocity(Feet/Sec)",{"v":236.539613199688,"d":"236.540"},{"v":240.84033343968233,"d":"240.840"},{"v":245.14105367967665,"d":"245.141"},{"v":249.441773919671,"d":"249.442"},{"v":253.74249415966534,"d":"253.742"},{"v":258.0432143996596,"d":"258.043"},{"v":262.3439346396539,"d":"262.344"},{"v":266.6446548796483,"d":"266.645"},{"v":270.9453751196426,"d":"270.945"},{"v":275.24609535963697,"d":"275.246"},{"v":279.54681559963126,"d":"279.547"},{"v":283.84753583962555,"d":"283.848"},{"v":288.14825607961996,"d":"288.148"},{"v":292.44897631961425,"d":"292.449"}]
[{"$nulls":6},"from Data Input-Results Spreadsheet",null,null,"  Gallon/Min",{"$nulls":3},"Gallon/Min",null,null,{"v":0.23661500743502015,"d":"0.24"},{"v":0.2409170984792933,"d":"0.24"},{"v":0.24521918952356636,"d":"0.25"},{"v":0.24952128056783943,"d":"0.25"},{"v":0.25382337161211255,"d":"0.25"},{"v":0.2581254626563856,"d":"0.26"},{"v":0.2624275537006587,"d":"0.26"},{"v":0.2667296447449318,"d":"0.27"},{"v":0.27103173578920486,"d":"0.27"},{"v":0.27533382683347796,"d":"0.28"},{"v":0.27963591787775105,"d":"0.28"},{"v":0.2839380089220242,"d":"0.28"},{"v":0.2882400999662973,"d":"0.29"},{"v":0.2925421910105704,"d":"0.29"},null,"Runner Air Velocity MPH",{"v":161.27700899978726,"d":"161.277"},{"v":164.20931825432888,"d":"164.209"},{"v":167.14162750887044,"d":"167.142"},{"v":170.07393676341204,"d":"170.074"},{"v":173.00624601795363,"d":"173.006"},{"v":175.93855527249517,"d":"175.939"},{"v":178.87086452703676,"d":"178.871"},{"v":181.80317378157835,"d":"181.803"},{"v":184.73548303611994,"d":"184.735"},{"v":187.6677922906616,"d":"187.668"},{"v":190.60010154520313,"d":"190.600"},{"v":193.5324107997447,"d":"193.532"},{"v":196.46472005428632,"d":"196.465"}]
[{"$nulls":8},"  ","  Gallon/Hour",{"$nulls":3},"Gallon/Hour",null,null,{"v":14.196900446101209,"d":"14.20"},{"v":14.455025908757598,"d":"14.46"},{"v":14.713151371413982,"d":"14.71"},{"v":14.971276834070366,"d":"14.97"},{"v":15.229402296726754,"d":"15.23"},{"v":15.487527759383134,"d":"15.49"},{"v":15.74565322203952,"d":"15.75"},{"v":16.00377868469591,"d":"16.00"},{"v":16.261904147352293,"d":"16.26"},{"v":16.520029610008677,"d":"16.52"},{"v":16.77815507266506,"d":"16.78"},{"v":17.036280535321453,"d":"17.04"},{"v":17.294405997977837,"d":"17.29"},{"v":17.552531460634224,"d":"17.55"},null,"Runner Air Velocity (inches/sec)",{"v":2838.475358396256,"d":"2838.475"},{"v":2890.084001276188,"d":"2890.084"},{"v":2941.69264415612,"d":"2941.693"},{"v":2993.3012870360517,"d":"2993.301"},{"v":3044.9099299159843,"d":"3044.910"},{"v":3096.518572795915,"d":"3096.519"},{"v":3148.127215675847,"d":"3148.127"},{"v":3199.7358585557795,"d":"3199.736"},{"v":3251.344501435711,"d":"3251.345"},{"v":3302.953144315644,"d":"3302.953"},{"v":3354.561787195575,"d":"3354.562"},{"v":3406.1704300755064,"d":"3406.170"},{"v":3457.7790729554395,"d":"3457.779"},{"v":3509.3877158353707,"d":"3509.388"}]
[]
[{"$nulls":9},"Power/Heat Calculations",{"$nulls":31},{"v":140.74074074074073,"d":"140.741"},"cfpm"]
[{"$nulls":9},"BTU/sec ",{"$nulls":3},"BTU/Second",null,null,{"v":449.5685141265383,"d":"450"},{"v":457.74248711065724,"d":"458"},{"v":465.9164600947761,"d":"466"},{"v":474.09043307889493,"d":"474"},{"v":482.26440606301384,"d":"482"},{"v":490.4383790471326,"d":"490"},{"v":498.6123520312514,"d":"499"},{"v":506.78632501537044,"d":"507"},{"v":514.9602979994893,"d":"515"},{"v":523.1342709836082,"d":"523"},{"v":531.308243967727,"d":"531"},{"v":539.482216951846,"d":"539"},{"v":547.6561899359648,"d":"548"},{"v":555.8301629200837,"d":"556"},{"$nulls":9},1.25,1.227184630308513,{"v":2.3456790123456788,"d":"2.346"},"cfps"]
[{"$nulls":9},"Torque Ft-lbs",{"$nulls":3},"Torque (Ft-Lbs)",null,null,{"v":349764.3039904468,"d":"349764"},{"v":356123.6549720913,"d":"356124"},{"v":362483.0059537358,"d":"362483"},{"v":368842.35693538026,"d":"368842"},{"v":375201.7079170248,"d":"375202"},{"v":381561.0588986692,"d":"381561"},{"v":387920.4098803136,"d":"387920"},{"v":394279.7608619582,"d":"394280"},{"v":400639.1118436027,"d":"400639"},{"v":406998.46282524714,"d":"406998"},{"v":413357.8138068916,"d":"413358"},{"v":419717.1647885362,"d":"419717"},{"v":426076.5157701806,"d":"426077"},{"v":432435.8667518251,"d":"432436"},{"$nulls":9},1.5,1.7671458676442586]
[{"$nulls":9},"Horse Power (Total)",{"$nulls":3},"Horse Power (Total)",null,null,{"v":635.9350981644487,"d":"636"},{"v":647.4975544947115,"d":"647"},{"v":659.0600108249741,"d":"659"},{"v":670.6224671552368,"d":"671"},{"v":682.1849234854997,"d":"682"},{"v":693.7473798157622,"d":"694"},{"v":705.3098361460247,"d":"705"},{"v":716.8722924762876,"d":"717"},{"v":728.4347488065503,"d":"728"},{"v":739.997205136813,"d":"740"},{"v":751.5596614670757,"d":"752"},{"v":763.1221177973385,"d":"763"},{"v":774.6845741276011,"d":"775"},{"v":786.2470304578638,"d":"786"},{"$nulls":9},"Area",2.9943304979527716]
[{"$nulls":8},"26","  Useful",{"v":0.24,"d":"24%"},{"v":24,"d":"24.000"},null,"Horse Power (Useful)",null,null,{"v":152.6244235594677,"d":"153"},{"v":155.39941307873076,"d":"155"},{"v":158.17440259799378,"d":"158"},{"v":160.94939211725682,"d":"161"},{"v":163.72438163651992,"d":"164"},{"v":166.4993711557829,"d":"166"},{"v":169.27436067504593,"d":"169"},{"v":172.04935019430903,"d":"172"},{"v":174.82433971357204,"d":"175"},{"v":177.59932923283512,"d":"178"},{"v":180.37431875209816,"d":"180"},{"v":183.14930827136124,"d":"183"},{"v":185.92429779062425,"d":"186"},{"v":188.69928730988732,"d":"189"},{"$nulls":9},"Area ft^2",0.020793961791338692,{"v":112.80577678673644,"d":"112.806"},"fps"]
[{"$nulls":9},"  Cooling Loss",{"v":0.26,"d":"26%"},{"v":26,"d":"26.000"},null,"HP Loss (Cooling)",null,null,{"v":165.34312552275668,"d":"165"},{"v":168.349364168625,"d":"168"},{"v":171.3556028144933,"d":"171"},{"v":174.36184146036157,"d":"174"},{"v":177.3680801062299,"d":"177"},{"v":180.3743187520982,"d":"180"},{"v":183.38055739796644,"d":"183"},{"v":186.38679604383478,"d":"186"},{"v":189.3930346897031,"d":"189"},{"v":192.3992733355714,"d":"192"},{"v":195.40551198143967,"d":"195"},{"v":198.41175062730804,"d":"198"},{"v":201.4179892731763,"d":"201"},{"v":204.4242279190446,"d":"204"}]
[{"$nulls":8},"40","  Exhaust Loss",{"v":0.5,"d":"50%"},{"v":50,"d":"50.000"},null,"HP Loss (Exhaust)",null,null,{"v":317.96754908222437,"d":"318"},{"v":323.74877724735575,"d":"324"},{"v":329.53000541248707,"d":"330"},{"v":335.3112335776184,"d":"335"},{"v":341.09246174274983,"d":"341"},{"v":346.8736899078811,"d":"347"},{"v":352.65491807301237,"d":"353"},{"v":358.4361462381438,"d":"358"},{"v":364.21737440327513,"d":"364"},{"v":369.9986025684065,"d":"370"},{"v":375.77983073353784,"d":"376"},{"v":381.5610588986693,"d":"382"},{"v":387.34228706380054,"d":"387"},{"v":393.1235152289319,"d":"393"}]
[]
[{"$nulls":4}," ",{"$nulls":4},"Cooling Requirements BTU/Min"]
[{"$nulls":9},"  Total Cooling Rejection BTU",{"$nulls":3},"Total BTU Rejection  BTU/Min",null,null,{"v":7013.268820373998,"d":"7013"},{"v":7140.782798926253,"d":"7141"},{"v":7268.296777478507,"d":"7268"},{"v":7395.810756030761,"d":"7396"},{"v":7523.324734583017,"d":"7523"},{"v":7650.83871313527,"d":"7651"},{"v":7778.352691687523,"d":"7778"},{"v":7905.866670239779,"d":"7906"},{"v":8033.380648792034,"d":"8033"},{"v":8160.894627344289,"d":"8161"},{"v":8288.408605896542,"d":"8288"},{"v":8415.9225844488,"d":"8416"},{"v":8543.436563001052,"d":"8543"},{"v":8670.950541553306,"d":"8671"}]
[{"$nulls":9},"  Radiator = 2/3 of  Rejection"," ",null,null,"BTU Rejection Radiators",null,null,{"v":4675.512546915998,"d":"4676"},{"v":4760.5218659508355,"d":"4761"},{"v":4845.531184985671,"d":"4846"},{"v":4930.540504020507,"d":"4931"},{"v":5015.549823055345,"d":"5016"},{"v":5100.55914209018,"d":"5101"},{"v":5185.568461125015,"d":"5186"},{"v":5270.577780159852,"d":"5271"},{"v":5355.5870991946895,"d":"5356"},{"v":5440.596418229526,"d":"5441"},{"v":5525.605737264362,"d":"5526"},{"v":5610.6150562992,"d":"5611"},{"v":5695.624375334035,"d":"5696"},{"v":5780.63369436887,"d":"5781"}]
[{"$nulls":9},"  Oil Cooler = 1/3 of Rejection",{"$nulls":3},"BTU Rejection Oil Cooler",null,null,{"v":2337.756273457999,"d":"2338"},{"v":2380.2609329754177,"d":"2380"},{"v":2422.7655924928354,"d":"2423"},{"v":2465.2702520102534,"d":"2465"},{"v":2507.7749115276724,"d":"2508"},{"v":2550.27957104509,"d":"2550"},{"v":2592.7842305625077,"d":"2593"},{"v":2635.288890079926,"d":"2635"},{"v":2677.7935495973447,"d":"2678"},{"v":2720.298209114763,"d":"2720"},{"v":2762.802868632181,"d":"2763"},{"v":2805.3075281496,"d":"2805"},{"v":2847.8121876670175,"d":"2848"},{"v":2890.316847184435,"d":"2890"}]
[]
[{"$nulls":9},"Injector timing "]
[{"$nulls":9},"  Total Fuel Flow Requirement Lbm/Min",{"$nulls":3},"Total Fuel flow Required (Lbm/min)",null,null,{"v":1.4196900446101208,"d":"1.42E+00"},{"v":1.4455025908757597,"d":"1.45E+00"},{"v":1.4713151371413982,"d":"1.47E+00"},{"v":1.4971276834070366,"d":"1.50E+00"},{"v":1.5229402296726753,"d":"1.52E+00"},{"v":1.5487527759383135,"d":"1.55E+00"},{"v":1.574565322203952,"d":"1.57E+00"},{"v":1.6003778684695908,"d":"1.60E+00"},{"v":1.6261904147352293,"d":"1.63E+00"},{"v":1.6520029610008677,"d":"1.65E+00"},{"v":1.6778155072665064,"d":"1.68E+00"},{"v":1.703628053532145,"d":"1.70E+00"},{"v":1.7294405997977838,"d":"1.73E+00"},{"v":1.7552531460634222,"d":"1.76E+00"}," "]
[{"$nulls":9},"  Fuel Required lbm/msec",{"$nulls":3},"Fuel Flow Required (Lbm/Millisecond)",null,null,2.3661500743502015e-05,2.409170984792933e-05,2.4521918952356635e-05,2.495212805678394e-05,2.5382337161211255e-05,2.5812546265638558e-05,2.6242755370065868e-05,2.667296447449318e-05,2.7103173578920488e-05,2.7533382683347798e-05,2.7963591787775108e-05,2.8393800892202415e-05,2.8824009996629728e-05,2.9254219101057035e-05," "]
[{"$nulls":9},"  On time Required per injector/msec",{"$nulls":3},"On-time per Injector (Millisecond)",null,null,{"v":4.732300148700403,"d":"4.73"},{"v":4.818341969585866,"d":"4.82"},{"v":4.904383790471327,"d":"4.90"},{"v":4.9904256113567875,"d":"4.99"},{"v":5.076467432242251,"d":"5.08"},{"v":5.162509253127711,"d":"5.16"},{"v":5.248551074013173,"d":"5.25"},{"v":5.334592894898636,"d":"5.33"},{"v":5.4206347157840975,"d":"5.42"},{"v":5.506676536669559,"d":"5.51"},{"v":5.592718357555021,"d":"5.59"},{"v":5.678760178440482,"d":"5.68"},{"v":5.764801999325945,"d":"5.76"},{"v":5.850843820211407,"d":"5.85"}," "]
[]
[{"$nulls":9},"Injection Set Up Parameters",{"$nulls":5}," "," ","Fuel Flow Required (Lbm/Millisecond) / Flow Rate (Lbm/Msec) per Injector * Factor for Number of Staged Injectors (Longer times for few injectors) * Inverse of Trigger Divide By"]
[{"$nulls":8},"These value","  Injectors Staged at (RPM) - User Value",null,{"v":3000,"d":"3000.000"},{"$nulls":3}," ","Injector On time ="]
[{"$nulls":8},"only need to","  Ignition Divide by (Haltech) otherwise 1",null,{"v":2,"d":"2.000"},{"$nulls":3}," "," "]
[{"$nulls":8},"be entered","  Injector Flow Rate per Injector Lbs/hr",null,{"v":45,"d":"45.000"}]
[{"$nulls":8},"once per","  80% max Flow Rate Lbs/hr",null,{"v":40.5,"d":"40.500"}]
[{"$nulls":8},"engine ","  Fuel Pressure actuall/45psi",null,40,{"v":0.8888888888888888,"d":"0.889"}]
[{"$nulls":8},"configuration","  Number of injectors",null,{"v":4,"d":"4.000"}]
[{"$nulls":9},"  Flow Rate Lbs/msec per Injector",null,{"v":1e-05,"d":"1.00E-05"}]
[{"$nulls":9}," ",null," "]
[{"$nulls":16}," "]
[{"$nulls":10}," ",{"$nulls":5}," "]
[{"$nulls":9},"Table for Adjusting Cooling Air density based on temp"]
[{"$nulls":8},"Air Density Adjustment (Actual/Standard Air Density)",null,"Temp F","Density","Ratio","Inverse/ratio"]
[{"$nulls":8},"Standard (59F at 29.92)",null,59,0.002378]
[{"$nulls":10},-15,0.00266,0.893984962406015,1.1185870479394449]
[{"$nulls":10},-10,0.00264,0.9007575757575758,1.1101766190075695]
[{"$nulls":10},-5,0.00262,0.9076335877862596,1.1017661900756939]
[{"$nulls":10},0,0.0026,0.9146153846153846,1.0933557611438183]
[{"$nulls":10},5,0.00258,0.9217054263565891,1.084945332211943]
[{"$nulls":10},10,0.0025599999999999998,0.92890625,1.0765349032800673]
[{"$nulls":10},15,0.0025399999999999997,0.936220472440945,1.0681244743481917]
[{"$nulls":10},20,0.0025199999999999997,0.9436507936507937,1.059714045416316]
[{"$nulls":10},25,0.0025,0.9511999999999999,1.0513036164844407,null,null," "]
[{"$nulls":10},30,0.00248,0.9588709677419355,1.042893187552565]
[{"$nulls":10},35,0.00246,0.9666666666666667,1.0344827586206897]
[{"$nulls":10},40,0.00244,0.9745901639344262,1.0260723296888141]
[{"$nulls":10},45,0.00242,0.9826446280991736,1.0176619007569385]
[{"$nulls":10},50,0.0024,0.9908333333333333,1.0092514718250631]
[{"$nulls":10},55,0.0023799999999999997,0.9991596638655463,1.0008410428931875]
[{"$nulls":10},60,0.002378,1,1]
[{"$nulls":10},65,0.00234,1.0162393162393162,0.9840201850294366]
[{"$nulls":10},70,0.00232,1.025,0.9756097560975611]
[{"$nulls":10},75,0.0023,1.0339130434782609,0.9671993271656855]
[{"$nulls":10},80,0.00228,1.042982456140351,0.9587888982338099]
[{"$nulls":10},85,0.00226,1.052212389380531,0.9503784693019343]
[{"$nulls":10},90,0.00224,1.061607142857143,0.9419680403700588]
[{"$nulls":10},95,0.0022199999999999998,1.0711711711711713,0.9335576114381832]
[{"$nulls":10},100,0.00221,1.0760180995475113,0.9293523969722456]

{"sheet":"Cooling Calculations","index":2,"n_rows":101,"n_cols":19,"rows_kept":101,"merged":[[0,3,1,3],[11,4,12,6],[19,3,20,3],[20,5,21,5],[33,3,34,3],[42,5,43,5]],"flags":["formulas_cached_only"]}
[" ","Choose Air Speed MPH","Climb Duct Speed Coef","True Air Speed MPH",null,"Radiator","Air Density at altitude =",0.076406092,"lb/ft^3","Cp Air","Cp Water","units Cp"]
["Indicated Air Speed =",120,0.3,null,"Ft/Sec","Area in^2","Area ft^2","Air Flow Cubic Feet Sec","Mass Flow Lb/min",0.25,1,"BTU/(Lbm* F)"]
["Engine rpm =",{"v":6000,"d":"6000.00"},"Radiators --->",36,{"v":52.8,"d":"52.80"},{"v":180,"d":"180.00"},1.25,{"v":66,"d":"66.00"},{"v":302.56812432,"d":"302.57"}," "]
["Altitude =",{"v":100,"d":"100.00"},"Oil cooler---->",null,{"v":52.8,"d":"52.80"},{"v":85.5,"d":"85.50"},{"v":0.59375,"d":"0.59"},{"v":31.349999999999998,"d":"31.35"},{"v":143.71985905199998,"d":"143.72"}," ",null," "]
[{"$nulls":6},"Default Values",null,null,"Default Values",null," "]
[null,"Note: Default values for Radiator dimensions",null,"Radiator","Width =",9,9,"Number of Rads =",2,2]
[null,"are for GM evaporator cores",null,null,"Height =",{"v":10,"d":"10.00"},10,"Number of Oil Coolers",1,1]
[null,"Default for Oil cooler is stock RX-7",null," Delta T Rad (F)","Radiator =",70,50]
[{"$nulls":3},"oil Cooler","Width =",{"v":19,"d":"19.00"},19]
[{"$nulls":4},"Height =",{"v":4.5,"d":"4.50"},{"v":4.5,"d":"4.50"},{"$nulls":3}," "]
[{"$nulls":3}," Delta T oil  (F)","Oil = ",70,50]
[{"$nulls":4},"Note: if you desire your coolant  flow rate proprational to Engine rpm,. Enter \" =C15\" (without quotation marks) "]
[null,"Pump Factor",185.85," ",{"$nulls":3},"Default Values",null," "]
[null,"Water Pump RPM","Flow gpm",null,"Pump Flow",{"v":38.095238095238095,"d":"38"},"Gallons/Minute ","15-40"]
[null,7080,{"v":38.095238095238095,"d":"38"}," ","Coolant DT ",16,"Degree F","10-15"]
[null," ",null,null,"Cp Coolant",0.7,"Range 0.6 -1.0",0.7,null," "]
[]
[{"$nulls":14}," "]
[null,null,"Air Flow","Both Radiators","Q Btu/min","W lb/min","Cp Btu/lbF","Tin_ F  ","Tout_ F"," "," "]
[" ",null,null,"Heat Rejection Capacity",5294.942175599999,{"v":302.56812432,"d":"302.57"},0.25,59,129]
[{"$nulls":5},"Needed Heat Rejection",null,null," "]
[{"$nulls":4},"Q Btu/Min",null,"Status","Excess Cooling Capacity"," "]
[{"$nulls":4},5294.942175599999,5100.55914209018,"Cooling",{"v":0.03811014206378991,"d":"3.81%"}]
[" ",{"$nulls":3}," "]
[{"$nulls":4}," ",{"$nulls":9},"HP","Fuel"]
[null,null,"Coolant",null," ",null," ",{"$nulls":7},{"v":166.4993711557829,"d":"166"},{"v":15.487527759383134,"d":"15.49"}]
[null,null," Pump Flow",null,null,"13B Pump"]
[{"$nulls":5},"Flow Rate Gallons/Min","Mass Flow lbm/min"]
[{"$nulls":5},38.095238095238095,317.7142857142857]
[{"$nulls":12},"AF =",12.65,null," ","Temp F =",59," "]
[{"$nulls":12},"Altitude =",100,null," ","Manifold",{"v":29,"d":"29.00"}," "]
[{"$nulls":12},"Gear Ratio ",2.17,null," ","RESULTS"," "," "]
[null," ",null,null,"Q Btu/Min","W lb/Min","Cp Btu/Lb-F (0.6 -1.0)","Tin_F","Tout_F",{"$nulls":4}," ",null," "," ","Radiator Cooler Heat Rejection Requirement BTU/Minute","Oil Cooler Heat Rejection Requirements BTU/Minute"]
[{"$nulls":3},"Heat Rejection Capacity",3558.4,{"v":317.7142857142857,"d":"317.71"},0.7,210,194,{"$nulls":3},"Engine RPM","Prop RPM",null,"Horse Power/Sec","Gallon/Hour"]
[{"$nulls":4},"Q Btu/Min","Increase Pump Flow?",{"$nulls":6}," "," ",null," "," ","Btu/Min","Btu/Min"]
[{"$nulls":4},3558.4,"Yes",{"$nulls":6},5500,{"v":2534.562211981567,"d":"2535"},null,{"v":152.6244235594677,"d":"153"},{"v":14.196900446101209,"d":"14.20"},{"v":4675.512546915998,"d":"4676"},{"v":2337.756273457999,"d":"2338"}]
[{"$nulls":4}," "," ",{"$nulls":6},5600,{"v":2580.6451612903224,"d":"2581"},null,{"v":155.39941307873076,"d":"155"},{"v":14.455025908757598,"d":"14.46"},{"v":4760.5218659508355,"d":"4761"},{"v":2380.2609329754177,"d":"2380"}]
[{"$nulls":4}," ",{"$nulls":7},5700,{"v":2626.7281105990783,"d":"2627"},null,{"v":158.17440259799378,"d":"158"},{"v":14.713151371413982,"d":"14.71"},{"v":4845.531184985671,"d":"4846"},{"v":2422.7655924928354,"d":"2423"}]
[{"$nulls":12},5800,{"v":2672.811059907834,"d":"2673"},null,{"v":160.94939211725682,"d":"161"},{"v":14.971276834070366,"d":"14.97"},{"v":4930.540504020507,"d":"4931"},{"v":2465.2702520102534,"d":"2465"}]
[{"$nulls":12},5900,{"v":2718.89400921659,"d":"2719"},null,{"v":163.72438163651992,"d":"164"},{"v":15.229402296726754,"d":"15.23"},{"v":5015.549823055345,"d":"5016"},{"v":2507.7749115276724,"d":"2508"}]
[null,null,"Air Flow","Oil Cooler","Q Btu/min","W lb/min","Cp Btu/lbF","Tin_ F","Tout_ F",{"$nulls":3},6000,{"v":2764.9769585253457,"d":"2765"},null,{"v":166.4993711557829,"d":"166"},{"v":15.487527759383134,"d":"15.49"},{"v":5100.55914209018,"d":"5101"},{"v":2550.27957104509,"d":"2550"}]
[{"$nulls":4},2515.0975334099994,{"v":143.71985905199998,"d":"143.72"},0.25,59,129,{"$nulls":3},6100,{"v":2811.0599078341015,"d":"2811"},null,{"v":169.27436067504593,"d":"169"},{"v":15.74565322203952,"d":"15.75"},{"v":5185.568461125015,"d":"5186"},{"v":2592.7842305625077,"d":"2593"}]
[{"$nulls":5},"Needed Heat Rejection",null,null," ",{"$nulls":3},6200,{"v":2857.1428571428573,"d":"2857"},null,{"v":172.04935019430903,"d":"172"},{"v":16.00377868469591,"d":"16.00"},{"v":5270.577780159852,"d":"5271"},{"v":2635.288890079926,"d":"2635"}]
[null," ",null,null,"Q Btu/Min",null,"Status","Excess Cooling Capacity"," ",{"$nulls":3},6300,{"v":2903.225806451613,"d":"2903"},null,{"v":174.82433971357204,"d":"175"},{"v":16.261904147352293,"d":"16.26"},{"v":5355.5870991946895,"d":"5356"},{"v":2677.7935495973447,"d":"2678"}]
[{"$nulls":4},2515.0975334099994,2550.27957104509,"OverHeat",{"v":-0.013795365039399677,"d":"-1.38%"},{"$nulls":4},6400,{"v":2949.308755760369,"d":"2949"},null,{"v":177.59932923283512,"d":"178"},{"v":16.520029610008677,"d":"16.52"},{"v":5440.596418229526,"d":"5441"},{"v":2720.298209114763,"d":"2720"}]
[{"$nulls":4}," ",{"$nulls":7},6500,{"v":2995.3917050691243,"d":"2995"},null,{"v":180.37431875209816,"d":"180"},{"v":16.77815507266506,"d":"16.78"},{"v":5525.605737264362,"d":"5526"},{"v":2762.802868632181,"d":"2763"}]
[{"$nulls":12},6600,{"v":3041.47465437788,"d":"3041"},null,{"v":183.14930827136124,"d":"183"},{"v":17.036280535321453,"d":"17.04"},{"v":5610.6150562992,"d":"5611"},{"v":2805.3075281496,"d":"2805"}]
[{"$nulls":12},6700,{"v":3087.557603686636,"d":"3088"},null,{"v":185.92429779062425,"d":"186"},{"v":17.294405997977837,"d":"17.29"},{"v":5695.624375334035,"d":"5696"},{"v":2847.8121876670175,"d":"2848"}]
[{"$nulls":12},6800,{"v":3133.6405529953918,"d":"3134"},null,{"v":188.69928730988732,"d":"189"},{"v":17.552531460634224,"d":"17.55"},{"v":5780.63369436887,"d":"5781"},{"v":2890.316847184435,"d":"2890"}]
[null,null," ","Over all System Cooling Satus"]
[null,null,"Total BTU of Cooling Capacity",null,7810.039709009999,"Btu/Min","The excessive cooling capacity of the radiators apparently"]
[null,null,"Total BTU of Heat Rejection Needed",null,7650.83871313527,"Btu/Min","enables them to reject some of the heat not rejected by the "]
[{"$nulls":6},"oil cooler"]
[null,null,"Excess Cooling Capacity =",null,{"v":0.020808306362726715,"d":"2.08%"},{"$nulls":6}," "]
[]
[null,null,"Deficient Cooling Capacity =",null,""]
[]
[{"$nulls":11}," "]
{"$rows_empty":40}
["Number radiators"]
[2]
[2]

{"sheet":"Manifold Pressure","index":3,"n_rows":30,"n_cols":14,"rows_kept":30,"hidden":true,"flags":["formulas_cached_only"]}
["AutoTune"]
[null,null,"MAP \"Hg","Map Kpa"]
[null,null,12,40.6283422459893,{"$nulls":6}," "]
[]
[null,null," ",null,null,"=0.039158*(D8*10-31)/((D7+459.7) )"]
[{"$nulls":3},"KPA",null,"air density Manifold","Air Density Altitude"]
[null,null,"Temp  F",59,"\"Hg","lbm/ft^3","lbm/ft^3"]
[null,null,"Map KPA",98.18516042780747,29,0.07424231728024296,0.076406092,null,"=IF(D8<40.6,2,4)"]
[null,null,"Map \"Hg",98.18516042780747,{"v":29,"d":"29.00"}," "," "]
[null,null,"plbm /ft^3",0.0765,null,false,{"$nulls":5},"lbm/time unit"]
[null,null,"Ncylinders",4,{"$nulls":3},"injectors",null,"Duty Cycle ","1 hour","1 sec","1 millsecond"]
[null,null,"CID",160,{"$nulls":3},"#",4,"Limit"]
[null,null,"inj lbm/hr",45,{"$nulls":3},"Rate lbm/hr",44.5489,{"v":1,"d":"100.00%"}]
[null,null,"# inj",1,{"$nulls":3},"Lbm Total 1 hr",178.1956,178.1956,178.1956,0.04949877777777778,{"v":4.9498777777777783e-05,"d":"4.94988E-05"}]
[null,null,"Air/Fuel Ratio",14.7,{"$nulls":5},"Gallons",29.164582651391164,0.008101272958719768,8.101272958719767e-06]
[null,null,"Req Fuel =",9.35277365586331,"millsecond","injector time","for 4 stroke engine"]
[]
[null,null,"Rotor No.",2," ",{"$nulls":8}," "]
[null,null,"E shaft rpm",null,"1 face fires for each 360 deg of e shaft rotation so for 720 deg 2 faces fire or 2 x 40 = 80 cid"]
[null,null,"Displacement/face",40,null,null,"Ve ="]
[null,null,"Faces",3,null,null,{"v":1,"d":"100.00%"},{"$nulls":6}," "]
[{"$nulls":3},"Total Displacement","CF disp","air mass lbm","air mass*Ve","Air/Fuel Ratio","Fuel Mass lbm","injection time"]
[null,null,"Air Volume ",80,0.046296296296296294,0.0034371443185297664,{"v":0.0034371443185297664,"d":"3.43714E-03"},12,{"v":0.00028642869321081387,"d":"2.86429E-04"},5.78658112522941,"millseconds each for all injectors"]
[{"$nulls":9}," ",null,null," "," "]
[{"$nulls":4},"CFM","lbm/min","lbm/sec",null,"lbm/millsecond",null,"X10",null,null," "]
[null,null,"RPM",2200,101.85185185185185,7.561717500765486,{"v":0.1260286250127581,"d":"1.26029E-01"},14.7,{"v":8.573375851208034e-06,"d":"8.57338E-06"},{"v":0.17320378878237688,"d":"1.73204E-01"},{"v":1.7320378878237688,"d":"1.73203789"}," "]
[{"$nulls":4},"Gal/min"," ",null,null,{"v":0.0841902702246288,"d":"8.41903E-02"},"HP"]
[{"$nulls":4},"gal/hour"," ",null,null,{"v":5.051416213477728,"d":"5.05"},56.11664193517985]
[{"$nulls":8}," "," "," "]
[{"$nulls":8}," "]

{"sheet":"Performance","index":4,"n_rows":3,"n_cols":6,"rows_kept":3,"hidden":true,"flags":["formulas_cached_only"]}
["Propeller","Pitch",null,"Prop Performance based on Pitch"]
[null,72,null,"Engine RPM","Prop RPM","True Air Speed"]
["True Air Speed =",120,null,{"v":6000,"d":"6000.00"},2764.9769585253457,188.52115626309177]