{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":1,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":22,"n_cols":11,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Engine","Lycoming IO-320-D1B, 160HP, ram air induction"]
["Prop","Hartzell 70\" constant speed"]
["MAP",18.2]
["RPM",2300]
["Pressure Alt",13300]
["OAT (deg C)",8]
["Fuel Cap (gal)",42]
["Reserve (gal)",5]
["Climb Fuel",5]
["Cruise Fuel",32]
[]
["GPH","Mixture","TAS (kts)","IAS (kts)","NM/gal","Stat. MPG","Range (nm)","Range (mi)","Cruise Endurance (hrs)","Comments","% PWR"]
[7.1,"80-90 ROP",183,144,25.774647887323944,29.640845070422532,824.7887323943662,948.507042253521,4.507042253521127,"Smooth",0.55]
[6.8,null,184,144,27.058823529411764,31.117647058823525,865.8823529411765,995.7647058823528,4.705882352941177,"Smooth",0.55]
[6.6,"50 ROP",184,144,27.87878787878788,32.060606060606055,892.1212121212121,1025.9393939393938,4.848484848484849,"Smooth",0.55]
[6.4,null,181,142,28.28125,32.5234375,905,1040.75,5,"Smooth",0.55]
[6.1,null,180,141,29.508196721311478,33.9344262295082,944.2622950819673,1085.9016393442623,5.245901639344263,"Smooth",0.55]
[6,null,179,140,29.833333333333332,34.30833333333333,954.6666666666666,1097.8666666666666,5.333333333333333,"Very light engine roughness",0.55]
[5.8,"Peak",176,138,30.344827586206897,34.89655172413793,971.0344827586207,1116.6896551724137,5.517241379310345,"Very light engine roughness",0.54375]
[5.6,null,175,137,31.250000000000004,35.9375,1000.0000000000001,1150,5.714285714285714,"Very light engine roughness",0.525]
[5.4,"10-20 LOP",169.708,133,31.427407407407404,36.14151851851851,1005.6770370370369,1156.5285925925923,5.925925925925926,"Engine roughness",0.50625]
[5.2,"20-30 LOP",159.5,125,30.673076923076923,35.27403846153846,981.5384615384615,1128.7692307692307,6.153846153846153,"Significant engine roughness",0.4875]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}