{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1904","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":35,"n_cols":8,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Power Settings  TSIO 550"]
[]
["ROP"]
[]
[null,"RPM"]
[null,2700,2600,2500,2400,2300,2200,2100]
["MP"]
[33,85.71428571428571,82.53968253968253,79.36507936507937,76.19047619047619,73.01587301587301,69.84126984126983,66.66666666666667]
[32.5,84.4155844155844,81.2890812890813,78.16257816257816,75.03607503607502,71.90957190957191,68.78306878306879,65.65656565656566]
[32,83.11688311688312,80.03848003848003,76.96007696007696,73.88167388167388,70.8032708032708,67.72486772486772,64.64646464646465]
[31.5,81.81818181818183,78.78787878787878,75.75757575757575,72.72727272727273,69.69696969696969,66.66666666666666,63.63636363636363]
[31,80.51948051948052,77.53727753727753,74.55507455507455,71.57287157287156,68.59066859066859,65.60846560846561,62.62626262626263]
[30.5,79.22077922077922,76.2866762866763,73.35257335257334,70.41847041847042,67.48436748436748,64.55026455026454,61.61616161616161]
[30,77.92207792207793,75.03607503607502,72.15007215007215,69.26406926406926,66.37806637806638,63.49206349206349,60.60606060606061]
[29.5,76.62337662337663,73.78547378547378,70.94757094757095,68.1096681096681,65.27176527176528,62.43386243386243,59.5959595959596]
[29,75.32467532467533,72.53487253487253,69.74506974506974,66.95526695526695,64.16546416546416,61.37566137566137,58.58585858585859]
[28.5,74.02597402597402,71.28427128427128,68.54256854256853,65.8008658008658,63.05916305916306,60.317460317460316,57.57575757575758]
[28,72.72727272727273,70.03367003367002,67.34006734006735,64.64646464646464,61.95286195286195,59.25925925925925,56.56565656565656]
[27.5,71.42857142857143,68.78306878306879,66.13756613756614,63.49206349206349,60.84656084656085,58.201058201058196,55.55555555555556]
[27,70.12987012987013,67.53246753246754,64.93506493506493,62.33766233766234,59.74025974025974,57.14285714285714,54.54545454545454]
[26.5,68.83116883116884,66.28186628186627,63.73256373256374,61.18326118326117,58.63395863395863,56.08465608465608,53.535353535353536]
[26,67.53246753246754,65.03126503126502,62.53006253006252,60.02886002886003,57.527657527657524,55.026455026455025,52.52525252525252]
[25.5,66.23376623376623,63.78066378066377,61.327561327561334,58.87445887445887,56.421356421356414,53.96825396825397,51.515151515151516]
[25,64.93506493506493,62.53006253006252,60.12506012506012,57.72005772005772,55.31505531505532,52.910052910052904,50.505050505050505]
[]
[]
["LOP"]
[null,null,"Gal/Hr"]
[null,80,19.047619047619047]
[null,75,17.857142857142858,null,"Based on 14.7 HP/GPH"]
[null,70,16.666666666666668]
[null,65,15.476190476190476]
[null,60,14.285714285714286]
[null,55,13.095238095238097]
[null,50,11.904761904761905]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}