{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1904","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":45,"n_cols":2,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Dynamic Pressure "]
["q=.5*rho*v^2     rho=.002377, v =(ft/sec),  q = #/sq.ft."]
[]
["Knots","#/sq.in."]
[]
[10,0.0023511409141250003]
[20,0.009404563656500001]
[30,0.021160268227125006]
[40,0.037618254626000006]
[50,0.058778522853125]
[60,0.08464107290850002]
[70,0.115205904792125]
[80,0.15047301850400002]
[90,0.19044241404412499]
[91,0.19469797909869124]
[100,0.2351140914125]
[110,0.284488050609125]
[120,0.3385642916340001]
[130,0.397342814487125]
[140,0.4608236191685]
[150,0.529006705678125]
[160,0.6018920740160001]
[170,0.6794797241821251]
[180,0.7617696561764999]
[190,0.8487618699991252]
[200,0.94045636565]
[210,1.036853143129125]
[220,1.1379522024365]
[230,1.2437535435721252]
[240,1.3542571665360004]
[250,1.4694630713281251]
[260,1.5893712579485]
[270,1.713981726397125]
[280,1.843294476674]
[290,1.977309508779125]
[300,2.1160268227125]
[310,2.259446418474125]
[320,2.4075682960640004]
[330,2.5603924554821247]
[340,2.7179188967285004]
[350,2.8801476198031253]
[360,3.0470786247059998]
[370,3.218711911437125]
[380,3.3950474799965007]
[390,3.5760853303841253]